canon_event=STRAIGHT_TRAVERSE line=1 x=0 y=0 z=0 a=0 b=0 c=0 u=0 v=0 w=0
canon_event=SET_FEED_RATE rate=60
canon_event=ARC_FEED line=3 first_end=1 second_end=1 first_axis=1 second_axis=0 rotation=-1 axis_end_point=0 a=0 b=0 c=0 u=0 v=0 w=0
canon_event=COMMENT: interpreter: IJK distance mode changed to absolute
canon_event=ARC_FEED line=5 first_end=0 second_end=0 first_axis=0 second_axis=1 rotation=1 axis_end_point=0 a=0 b=0 c=0 u=0 v=0 w=0
canon_event=ARC_FEED line=6 first_end=1 second_end=0 first_axis=0.5 second_axis=-3.06162e-17 rotation=-1 axis_end_point=0 a=0 b=0 c=0 u=0 v=0 w=0
canon_event=STRAIGHT_TRAVERSE line=7 x=0 y=0 z=0 a=0 b=0 c=0 u=0 v=0 w=0
canon_event=ARC_FEED line=9 first_end=1 second_end=1 first_axis=0 second_axis=1 rotation=-1 axis_end_point=0 a=0 b=0 c=0 u=0 v=0 w=0
canon_event=STRAIGHT_TRAVERSE line=10 x=0 y=0 z=0 a=0 b=0 c=0 u=0 v=0 w=0
canon_event=ARC_FEED line=11 first_end=1 second_end=1 first_axis=0 second_axis=1 rotation=1 axis_end_point=0 a=0 b=0 c=0 u=0 v=0 w=0
canon_event=STRAIGHT_TRAVERSE line=12 x=0 y=0 z=0 a=0 b=0 c=0 u=0 v=0 w=0
canon_event=ARC_FEED line=13 first_end=1 second_end=0 first_axis=0.5 second_axis=0.866025 rotation=-1 axis_end_point=2 a=0 b=0 c=0 u=0 v=0 w=0
