execute_line_1=5
error_text=Cannot do g1 with zero feed rate
setup.current_x=0
setup.current_y=0
setup.current_z=0
setup.parameter_5420=0
setup.parameter_5421=0
setup.parameter_5422=0
absent=canon_event=STRAIGHT_FEED
