canon_event=SELECT_PLANE plane=1
canon_event=STRAIGHT_TRAVERSE line=1 x=0 y=0 z=0 a=0 b=0 c=0 u=0 v=0 w=0
canon_event=COMMENT: interpreter: feed mode set to inverse time
canon_event=SET_FEED_MODE spindle=0 mode=0
canon_event=COMMENT: interpreter: feed mode set to units per minute
canon_event=SET_FEED_MODE spindle=0 mode=0
canon_event=SET_FEED_RATE rate=0
canon_event=COMMENT: interpreter: feed mode set to units per revolution
canon_event=SET_FEED_MODE spindle=0 mode=1
canon_event=SET_FEED_RATE rate=0
canon_event=SET_MOTION_CONTROL_MODE mode=2 tolerance=0
canon_event=SET_MOTION_CONTROL_MODE mode=1 tolerance=0
canon_event=SET_MOTION_CONTROL_MODE mode=3 tolerance=0.02
canon_event=SET_NAIVECAM_TOLERANCE tolerance=0.03
setup.current_x=0
setup.current_y=0
setup.current_z=0
setup.parameter_5420=0
setup.parameter_5421=0
setup.parameter_5422=0
post_execute.plane=1
post_execute.distance_mode=0
post_execute.feed_mode=2
post_execute.motion_mode=0
post_execute.origin_index=0
post_execute.feed_override=0
post_execute.speed_override_0=0
post_execute.spindle_turning_0=1
post_execute.mist=0
post_execute.flood=0
