; Repeatedly move to 0,0,0 and 1,2,3 in machine coordinates,
; but with different offsets in effect; check that in each case,
; the values in #544x match the just-commanded g53 move
o<coords> sub
g53g0x0y0z0
(debug,#<_abs_x> #<_abs_y> #<_abs_z>)
g53g0x1y2z3
(debug,#<_abs_x> #<_abs_y> #<_abs_z>)
o<coords> endsub

o<suite> sub
g54
g92.2
g10l2p1x0y0z0r0
o<coords> call

g10l2p1x3y7z0r0
o<coords> call

g10l2p1x0y0r45
o<coords> call

g10l2p1x3y7z0r45
o<coords> call

g10l2p1x0y0z0r0
g92x3y7
o<coords> call
g92.2

g10l2p1x3y7z0r0
g92x3y7
o<coords> call
g92.2

g10l2p1x3y7z0r45
g92x3y7
o<coords> call
g92.2
o<suite> endsub

g20
o<suite> call

g21
o<suite> call

m2
