test_linuxcnc_source RUN 功能测试报告
测试对象：http://127.0.0.1:40261/web-rtcp-5axis-sim-plan/app/index.html
生成时间：2026-06-23 07:39:18 UTC

1. 测试结论
本次使用 working_run/test_linuxcnc_source 中的 INI 与 G-code 文件执行 RUN 测试，结果：PASS。
	检查项
	结果
	证据

	test_linuxcnc_source INI used
	PASS
	configs/sim/axis/vismach/5axis/table-rotary-tilting/xyzac-trt.ini

	test_linuxcnc_source G-code hash matches loaded source
	PASS
	e90f0b4b6c43809da94a8170ee1029b5afc3e1bbe9bf2ae66298a8baefad013c

	刀具路径预览点可见
	PASS
	pathPoints=4492

	刀具路径使用完整 canonical motion 点
	PASS
	threePathPoints=4492, motionEventCount=4492

	TCP/刀轴线可见
	PASS
	tcp=sphere, axis=line

	RUN 采样数量
	PASS
	samples=6

	每行执行高亮同步
	PASS
	9/9, 10/10, 11/11, 12/12, 12/12, 13/13

	程序列表显示每行执行过程
	PASS
	9:running:true, 10:running:true, 11:running:true, 12:running:true, 12:running:true, 13:running:true

	执行轨迹可见
	PASS
	1/ok, 1/ok, 1/ok, 1/ok, 1/ok, 1/ok

	实时轴值来自 task/HAL feedback
	PASS
	linuxcnc-task-motion-hal-wasm/true, linuxcnc-task-motion-hal-wasm/true, linuxcnc-task-motion-hal-wasm/true, linuxcnc-task-motion-hal-wasm/true, linuxcnc-task-motion-hal-wasm/true, linuxcnc-task-motion-hal-wasm/true

	RUN feed 不是固定 3600 mm/min
	PASS
	200ms=2100, 500ms=635.748, 1000ms=283.9176, 2000ms=59.12256, 5000ms=59.12256, 17000ms=58.19616

	RUN feed 随实际 G-code F/G93 段变化
	PASS
	2100, 635.748, 283.918, 59.123, 58.196

	RUN 使用 G93 inverse-time feed
	PASS
	200ms F4500000 inverse-time 0.4571722972663097s, 500ms F318 inverse-time 0.18867924528301888s, 1000ms F159 inverse-time 0.37735849056603776s, 2000ms F159 inverse-time 0.37735849056603776s, 5000ms F159 inverse-time 0.37735849056603776s, 17000ms F159 inverse-time 0.37735849056603776s

	task/HAL cycle 推进
	PASS
	35/350, 60/600, 85/850, 110/1100, 135/1350, 155/1550

	STOP 后 loop 停止
	PASS
	active=false, stopReason=stopped


2. 测试源文件
	项目
	内容

	INI
	/home/meswork/cnc_wams/web-rtcp-5axis-sim-plan/working_run/test_linuxcnc_source/xyzac-trt.ini

	INI SHA-256
	4b7fa6cb8d3e7031e769b3e0c779b586b67cfd45d715985f40d4ec23c662dc97

	G-code
	/home/meswork/cnc_wams/web-rtcp-5axis-sim-plan/working_run/test_linuxcnc_source/impeller-7bl-xyzac.ngc

	G-code SHA-256
	e90f0b4b6c43809da94a8170ee1029b5afc3e1bbe9bf2ae66298a8baefad013c

	G-code 行数/字节
	4511 / 294411


3. 测试过程
01-initial-ui - 初始界面
确认浏览器应用、五轴预览区、G-code 区和 DRO 面板已渲染。
	项目
	内容

	activeProgram
	configs/sim/axis/vismach/5axis/table-rotary-tilting/demos/boat-xyzac.ngc

	runState / activeLine
	idle / 1

	program source
	linuxcnc-vendored-5axis-gcode / linuxcnc-task-motion-hal-wasm

	selected G-code
	configs/sim/axis/vismach/5axis/table-rotary-tilting/demos/boat-xyzac.ngc

	task/HAL program
	/work/sim/axis/vismach/5axis/table-rotary-tilting/xyzac-trt/demos/boat-xyzac.ngc

	DRO XYZAC
	X=0.000 Y=0.000 Z=0.000 A=0.000 B=0.000 C=0.000

	axisPose XYZAC
	X=0.000 Y=0.000 Z=0.000 A=0.000 B=0.000 C=0.000

	path/executed
	2 / 1

	RTCP / kins
	on / tcp-xyzac

	pixel
	luma=128.52, nonBlack=0.7817


[image: ]
截图文件：/home/meswork/cnc_wams/qa/web-rtcp-5axis-site-test/screenshots/test-linuxcnc-source-run/01-initial-ui.png
02-stage-test-ini - Stage test_linuxcnc_source INI
使用 working_run/test_linuxcnc_source/xyzac-trt.ini 重新 staging machine files。
	项目
	内容

	activeProgram
	configs/sim/axis/vismach/5axis/table-rotary-tilting/demos/boat-xyzac.ngc

	runState / activeLine
	idle / 1

	program source
	linuxcnc-vendored-5axis-gcode / linuxcnc-task-motion-hal-wasm

	selected G-code
	-

	task/HAL program
	/work/sim/axis/vismach/5axis/table-rotary-tilting/xyzac-trt/demos/xyzac_switchkins.ngc

	DRO XYZAC
	X=0.000 Y=0.000 Z=0.000 A=0.000 B=0.000 C=0.000

	axisPose XYZAC
	X=0.000 Y=0.000 Z=0.000 A=0.000 B=0.000 C=0.000

	path/executed
	2 / 1

	RTCP / kins
	on / tcp-xyzac

	pixel
	luma=128.59, nonBlack=0.7817


[image: ]
截图文件：/home/meswork/cnc_wams/qa/web-rtcp-5axis-site-test/screenshots/test-linuxcnc-source-run/02-stage-test-ini.png
03-toolpath-preview - 刀具路径预览
加载 test_linuxcnc_source/impeller-7bl-xyzac.ngc 对应程序，确认 canonical motion 预览路径、TCP 球和刀轴线可见。
	项目
	内容

	activeProgram
	configs/sim/axis/vismach/5axis/table-rotary-tilting/demos/impeller-7bl-xyzac.ngc

	runState / activeLine
	idle / 1

	program source
	linuxcnc-vendored-5axis-gcode / linuxcnc-task-motion-hal-wasm

	selected G-code
	configs/sim/axis/vismach/5axis/table-rotary-tilting/demos/impeller-7bl-xyzac.ngc

	task/HAL program
	/work/sim/axis/vismach/5axis/table-rotary-tilting/xyzac-trt/demos/impeller-7bl-xyzac.ngc

	DRO XYZAC
	X=0.000 Y=0.000 Z=0.000 A=0.000 B=0.000 C=0.000

	axisPose XYZAC
	X=0.000 Y=0.000 Z=0.000 A=0.000 B=0.000 C=0.000

	path/executed
	4492 / 1

	RTCP / kins
	on / tcp-xyzac

	pixel
	luma=127.63, nonBlack=0.7643


[image: ]
截图文件：/home/meswork/cnc_wams/qa/web-rtcp-5axis-site-test/screenshots/test-linuxcnc-source-run/03-toolpath-preview.png
04-ready-before-run - RUN 前准备
POWER ON、HOME、AUTO、TCP 模式就绪，RUN gate 所需条件已满足。
	项目
	内容

	activeProgram
	configs/sim/axis/vismach/5axis/table-rotary-tilting/demos/impeller-7bl-xyzac.ngc

	runState / activeLine
	idle / 1

	program source
	linuxcnc-vendored-5axis-gcode / linuxcnc-task-motion-hal-wasm

	selected G-code
	configs/sim/axis/vismach/5axis/table-rotary-tilting/demos/impeller-7bl-xyzac.ngc

	task/HAL program
	/work/sim/axis/vismach/5axis/table-rotary-tilting/xyzac-trt/demos/impeller-7bl-xyzac.ngc

	DRO XYZAC
	X=0.000 Y=0.000 Z=0.000 A=0.000 B=0.000 C=0.000

	axisPose XYZAC
	X=0.000 Y=0.000 Z=0.000 A=0.000 B=0.000 C=0.000

	path/executed
	4492 / 1

	RTCP / kins
	on / tcp-xyzac

	pixel
	luma=127.67, nonBlack=0.7643


[image: ]
截图文件：/home/meswork/cnc_wams/qa/web-rtcp-5axis-site-test/screenshots/test-linuxcnc-source-run/04-ready-before-run.png
05-run-0200ms - G-code 执行 200ms
采集 G-code 当前高亮行、执行轨迹、实时 DRO/axisPose 和 task/HAL feedback。
	项目
	内容

	activeProgram
	configs/sim/axis/vismach/5axis/table-rotary-tilting/demos/impeller-7bl-xyzac.ngc

	runState / activeLine
	running / 9

	program source
	linuxcnc-vendored-5axis-gcode / linuxcnc-task-motion-hal-wasm

	selected G-code
	configs/sim/axis/vismach/5axis/table-rotary-tilting/demos/impeller-7bl-xyzac.ngc

	task/HAL program
	/work/sim/axis/vismach/5axis/table-rotary-tilting/xyzac-trt/demos/impeller-7bl-xyzac.ngc

	DRO XYZAC
	X=10.484 Y=-17.330 Z=30.081 A=-71.841 B=0.000 C=-35.930

	axisPose XYZAC
	X=10.484 Y=-17.330 Z=30.081 A=-71.841 B=0.000 C=-35.930

	path/executed
	4492 / 1

	RTCP / kins
	on / tcp-xyzac

	pixel
	luma=130.81, nonBlack=0.765


[image: ]
截图文件：/home/meswork/cnc_wams/qa/web-rtcp-5axis-site-test/screenshots/test-linuxcnc-source-run/05-run-0200ms.png
05-run-0500ms - G-code 执行 500ms
采集 G-code 当前高亮行、执行轨迹、实时 DRO/axisPose 和 task/HAL feedback。
	项目
	内容

	activeProgram
	configs/sim/axis/vismach/5axis/table-rotary-tilting/demos/impeller-7bl-xyzac.ngc

	runState / activeLine
	running / 10

	program source
	linuxcnc-vendored-5axis-gcode / linuxcnc-task-motion-hal-wasm

	selected G-code
	configs/sim/axis/vismach/5axis/table-rotary-tilting/demos/impeller-7bl-xyzac.ngc

	task/HAL program
	/work/sim/axis/vismach/5axis/table-rotary-tilting/xyzac-trt/demos/impeller-7bl-xyzac.ngc

	DRO XYZAC
	X=6.868 Y=-12.341 Z=28.059 A=-71.841 B=0.000 C=-35.930

	axisPose XYZAC
	X=6.868 Y=-12.341 Z=28.059 A=-71.841 B=0.000 C=-35.930

	path/executed
	4492 / 1

	RTCP / kins
	on / tcp-xyzac

	pixel
	luma=130.59, nonBlack=0.7649


[image: ]
截图文件：/home/meswork/cnc_wams/qa/web-rtcp-5axis-site-test/screenshots/test-linuxcnc-source-run/05-run-0500ms.png
05-run-1000ms - G-code 执行 1000ms
采集 G-code 当前高亮行、执行轨迹、实时 DRO/axisPose 和 task/HAL feedback。
	项目
	内容

	activeProgram
	configs/sim/axis/vismach/5axis/table-rotary-tilting/demos/impeller-7bl-xyzac.ngc

	runState / activeLine
	running / 11

	program source
	linuxcnc-vendored-5axis-gcode / linuxcnc-task-motion-hal-wasm

	selected G-code
	configs/sim/axis/vismach/5axis/table-rotary-tilting/demos/impeller-7bl-xyzac.ngc

	task/HAL program
	/work/sim/axis/vismach/5axis/table-rotary-tilting/xyzac-trt/demos/impeller-7bl-xyzac.ngc

	DRO XYZAC
	X=6.325 Y=-11.911 Z=27.104 A=-71.606 B=0.000 C=-34.700

	axisPose XYZAC
	X=6.325 Y=-11.911 Z=27.104 A=-71.606 B=0.000 C=-34.700

	path/executed
	4492 / 1

	RTCP / kins
	on / tcp-xyzac

	pixel
	luma=130.48, nonBlack=0.7649


[image: ]
截图文件：/home/meswork/cnc_wams/qa/web-rtcp-5axis-site-test/screenshots/test-linuxcnc-source-run/05-run-1000ms.png
05-run-2000ms - G-code 执行 2000ms
采集 G-code 当前高亮行、执行轨迹、实时 DRO/axisPose 和 task/HAL feedback。
	项目
	内容

	activeProgram
	configs/sim/axis/vismach/5axis/table-rotary-tilting/demos/impeller-7bl-xyzac.ngc

	runState / activeLine
	running / 12

	program source
	linuxcnc-vendored-5axis-gcode / linuxcnc-task-motion-hal-wasm

	selected G-code
	configs/sim/axis/vismach/5axis/table-rotary-tilting/demos/impeller-7bl-xyzac.ngc

	task/HAL program
	/work/sim/axis/vismach/5axis/table-rotary-tilting/xyzac-trt/demos/impeller-7bl-xyzac.ngc

	DRO XYZAC
	X=6.357 Y=-12.431 Z=26.155 A=-71.258 B=0.000 C=-32.875

	axisPose XYZAC
	X=6.357 Y=-12.431 Z=26.155 A=-71.258 B=0.000 C=-32.875

	path/executed
	4492 / 1

	RTCP / kins
	on / tcp-xyzac

	pixel
	luma=130.47, nonBlack=0.7649


[image: ]
截图文件：/home/meswork/cnc_wams/qa/web-rtcp-5axis-site-test/screenshots/test-linuxcnc-source-run/05-run-2000ms.png
05-run-5000ms - G-code 执行 5000ms
采集 G-code 当前高亮行、执行轨迹、实时 DRO/axisPose 和 task/HAL feedback。
	项目
	内容

	activeProgram
	configs/sim/axis/vismach/5axis/table-rotary-tilting/demos/impeller-7bl-xyzac.ngc

	runState / activeLine
	running / 12

	program source
	linuxcnc-vendored-5axis-gcode / linuxcnc-task-motion-hal-wasm

	selected G-code
	configs/sim/axis/vismach/5axis/table-rotary-tilting/demos/impeller-7bl-xyzac.ngc

	task/HAL program
	/work/sim/axis/vismach/5axis/table-rotary-tilting/xyzac-trt/demos/impeller-7bl-xyzac.ngc

	DRO XYZAC
	X=6.349 Y=-12.557 Z=25.943 A=-71.187 B=0.000 C=-32.468

	axisPose XYZAC
	X=6.349 Y=-12.557 Z=25.943 A=-71.187 B=0.000 C=-32.468

	path/executed
	4492 / 1

	RTCP / kins
	on / tcp-xyzac

	pixel
	luma=130.45, nonBlack=0.7648


[image: ]
截图文件：/home/meswork/cnc_wams/qa/web-rtcp-5axis-site-test/screenshots/test-linuxcnc-source-run/05-run-5000ms.png
05-run-17000ms - G-code 执行 17000ms
采集 G-code 当前高亮行、执行轨迹、实时 DRO/axisPose 和 task/HAL feedback。
	项目
	内容

	activeProgram
	configs/sim/axis/vismach/5axis/table-rotary-tilting/demos/impeller-7bl-xyzac.ngc

	runState / activeLine
	running / 13

	program source
	linuxcnc-vendored-5axis-gcode / linuxcnc-task-motion-hal-wasm

	selected G-code
	configs/sim/axis/vismach/5axis/table-rotary-tilting/demos/impeller-7bl-xyzac.ngc

	task/HAL program
	/work/sim/axis/vismach/5axis/table-rotary-tilting/xyzac-trt/demos/impeller-7bl-xyzac.ngc

	DRO XYZAC
	X=6.336 Y=-12.659 Z=25.777 A=-71.141 B=0.000 C=-32.149

	axisPose XYZAC
	X=6.336 Y=-12.659 Z=25.777 A=-71.141 B=0.000 C=-32.149

	path/executed
	4492 / 1

	RTCP / kins
	on / tcp-xyzac

	pixel
	luma=130.44, nonBlack=0.765


[image: ]
截图文件：/home/meswork/cnc_wams/qa/web-rtcp-5axis-site-test/screenshots/test-linuxcnc-source-run/05-run-17000ms.png
06-stop-after-run - STOP 后状态
停止 RUN，确认 status loop 停止且执行证据已保留。
	项目
	内容

	activeProgram
	configs/sim/axis/vismach/5axis/table-rotary-tilting/demos/impeller-7bl-xyzac.ngc

	runState / activeLine
	stopped / 13

	program source
	linuxcnc-vendored-5axis-gcode / linuxcnc-task-motion-hal-wasm

	selected G-code
	configs/sim/axis/vismach/5axis/table-rotary-tilting/demos/impeller-7bl-xyzac.ngc

	task/HAL program
	/work/sim/axis/vismach/5axis/table-rotary-tilting/xyzac-trt/demos/impeller-7bl-xyzac.ngc

	DRO XYZAC
	X=6.331 Y=-12.685 Z=25.737 A=-71.132 B=0.000 C=-32.071

	axisPose XYZAC
	X=6.331 Y=-12.685 Z=25.737 A=-71.132 B=0.000 C=-32.071

	path/executed
	4492 / 1

	RTCP / kins
	on / tcp-xyzac

	pixel
	luma=130.4, nonBlack=0.7647


[image: ]
截图文件：/home/meswork/cnc_wams/qa/web-rtcp-5axis-site-test/screenshots/test-linuxcnc-source-run/06-stop-after-run.png
4. RUN 采样明细
	时间
	行号
	状态
	DRO XYZAC
	速度/feed
	轨迹点
	反馈

	200ms
	9 / UI 9
	running
	X=10.484 Y=-17.330 Z=30.081 A=-71.841 B=0.000 C=-35.930
	2100 mm/min
F4500000 inverse-time
	1
	linuxcnc-task-motion-hal-wasm
cycle=35/350

	500ms
	10 / UI 10
	running
	X=6.868 Y=-12.341 Z=28.059 A=-71.841 B=0.000 C=-35.930
	635.748 mm/min
F318 inverse-time
	1
	linuxcnc-task-motion-hal-wasm
cycle=60/600

	1000ms
	11 / UI 11
	running
	X=6.325 Y=-11.911 Z=27.104 A=-71.606 B=0.000 C=-34.700
	283.9176 mm/min
F159 inverse-time
	1
	linuxcnc-task-motion-hal-wasm
cycle=85/850

	2000ms
	12 / UI 12
	running
	X=6.357 Y=-12.431 Z=26.155 A=-71.258 B=0.000 C=-32.875
	59.12256 mm/min
F159 inverse-time
	1
	linuxcnc-task-motion-hal-wasm
cycle=110/1100

	5000ms
	12 / UI 12
	running
	X=6.349 Y=-12.557 Z=25.943 A=-71.187 B=0.000 C=-32.468
	59.12256 mm/min
F159 inverse-time
	1
	linuxcnc-task-motion-hal-wasm
cycle=135/1350

	17000ms
	13 / UI 13
	running
	X=6.336 Y=-12.659 Z=25.777 A=-71.141 B=0.000 C=-32.149
	58.19616 mm/min
F159 inverse-time
	1
	linuxcnc-task-motion-hal-wasm
cycle=155/1550


5. 原始证据
	项目
	内容

	JSON
	/home/meswork/cnc_wams/qa/web-rtcp-5axis-site-test/output/test-linuxcnc-source-run-report.json

	截图目录
	/home/meswork/cnc_wams/qa/web-rtcp-5axis-site-test/screenshots/test-linuxcnc-source-run

	Word
	/home/meswork/cnc_wams/qa/web-rtcp-5axis-site-test/output/test-linuxcnc-source-run-report-2026-06-23.docx

	Console error
	2

	Chrome
	/usr/bin/google-chrome


6. Console Error
Failed to load resource: the server responded with a status of 404 (Not Found)
Failed to load resource: the server responded with a status of 404 (Not Found)
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